**Journal #2 - Samsung s III**

* *Nov 21, 2024*

**PostmarketOS**




Research possible solution ([postmarketOS-wiki](https://wiki.postmarketos.org/wiki/Samsung_Galaxy_S_III_(samsung-m0)#Installation%5C))

1. Flash an SD card


* *Download the compressed software image file*

For this section, you’ll need to select your preferred interface from the ones provided on postmarketOS site ([postmarketOS-interface-versions](https://images.postmarketos.org/bpo/v24.06/samsung-m0/))


* [Gnome-mobile](https://images.postmarketos.org/bpo/v24.06/samsung-m0/gnome-mobile/) - Chosen option, since we are more familiar with Gnome interface




* [Phosh](https://images.postmarketos.org/bpo/v24.06/samsung-m0/phosh/) - version derived from Gnome



* [Plasma-mobile](https://images.postmarketos.org/bpo/v24.06/samsung-m0/plasma-mobile/) - Appearance similar to typical Android Distributions, still ugly



* [Sxmo-de-sway](https://images.postmarketos.org/bpo/v24.06/samsung-m0/sxmo-de-sway/) - Lacking visual documentation, Personally unappealing as it feels more like operating a computer rather than a mobile device



* Extract the software image file
* Connect the SD Card to the computer
* Verify the software image file (Optional)
* Format the SD Card (Optional)
* Flash the SD Card
* [Gnome-mobile](https://images.postmarketos.org/bpo/v24.06/samsung-m0/gnome-mobile/)
* [Phosh](https://images.postmarketos.org/bpo/v24.06/samsung-m0/phosh/)
* [Plasma-mobile](https://images.postmarketos.org/bpo/v24.06/samsung-m0/plasma-mobile/)
* [sxmo-de-sway](https://images.postmarketos.org/bpo/v24.06/samsung-m0/sxmo-de-sway/)